<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="50" y1="8" x2="50" y2="50" width="0" layer="20"/>
<wire x1="50" y1="50" x2="0" y2="50" width="0" layer="20"/>
<wire x1="0" y1="50" x2="0" y2="0" width="0" layer="20"/>
<wire x1="50" y1="8" x2="19.75" y2="8" width="0" layer="20"/>
<text>PEXternalizer 0.9
@securelyfitz's Pci Express eXternalizer
https://github.com/securelyfitz/PEXternalizer</text>
<text>PEXternalizer 0.9
@securelyfitz's Pci Express eXternalizer
https://github.com/securelyfitz/PEXternalizer</text>
<text>PEXternalizer 0.9</text>
<text>PEXternalizer 0.9</text>
<text>Joe FitzPatrick
joefitz@securinghardware.com
@securelyfitz
213.373.4892</text>
</plain>
<libraries>
<library name="con-pci_express%28pci-e%29">
<description>PCI-Express 16x  connectors, 164 contacts  (2*82)
Included: Trough-hole connector and edge-card pattern

Manufacturer: FCI  Reference: 10018783-10113TLF

Reference Radiospares: 615-9530 
Reference Digikey: 609-1975-ND</description>
<packages>
<package name="USB3_FLAT">
</package>
<package name="PCI-E_36_CONN">
</package>
<package name="PCI-E_36_EDGE">
</package>
</packages>
</library>
<library name="con-molex">
<description>&lt;b&gt;Molex Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="22-23-2031">
<description>.100" (2.54mm) Center Header - 3 Pin</description>
</package>
<package name="22-23-2041">
<description>.100" (2.54mm) Center Header - 4 Pin</description>
</package>
</packages>
</library>
<library name="capacitor-wima">
<description>&lt;b&gt;WIMA Capacitors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="C5B2.5">
<description>&lt;B&gt;MKS2&lt;/B&gt;, 7.5 x 2.5 mm, grid 5.08 mm</description>
</package>
<package name="C2.5-2">
<description>&lt;B&gt;MKS2&lt;/B&gt;, 5 x 2.5 mm, grid 2.54 mm</description>
</package>
</packages>
</library>
<library name="securinghardware">
<packages>
<package name="SH">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="con-pci_express%28pci-e%29" package="USB3_FLAT" value="USB3FLAT"/>
<element name="3.3V" library="con-pci_express%28pci-e%29" package="PCI-E_36_EDGE" value="PCI-E1XEDGE"/>
<element name="U$2" library="con-pci_express%28pci-e%29" package="USB3_FLAT" value="USB3FLAT"/>
<element name="3.3V1" library="con-pci_express%28pci-e%29" package="PCI-E_36_CONN" value="PCI-E1XCONN"/>
<element name="X1" library="con-molex" package="22-23-2031" value="22-23-2031">
<attribute name="OC_NEWARK" value="30C0862"/>
<attribute name="MPN" value="22-23-2031"/>
<attribute name="MF" value="MOLEX"/>
<attribute name="OC_FARNELL" value="1462950"/>
</element>
<element name="C1" library="capacitor-wima" package="C5B2.5" value="100uF"/>
<element name="C2" library="capacitor-wima" package="C5B2.5" value="100uF"/>
<element name="C3" library="capacitor-wima" package="C2.5-2" value="100uF"/>
<element name="X2" library="con-molex" package="22-23-2041" value="22-23-2041">
<attribute name="OC_NEWARK" value="38C0355"/>
<attribute name="MPN" value="22-23-2041"/>
<attribute name="MF" value="MOLEX"/>
<attribute name="OC_FARNELL" value="1462920"/>
</element>
<element name="U$3" library="securinghardware" package="SH" value=""/>
<element name="U$4" library="securinghardware" package="SH" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="U$1" pad="7"/>
<contactref element="3.3V" pad="A18"/>
<contactref element="3.3V" pad="A15"/>
<contactref element="3.3V" pad="A12"/>
<contactref element="3.3V" pad="A4"/>
<contactref element="3.3V" pad="B4"/>
<contactref element="3.3V" pad="B7"/>
<contactref element="3.3V" pad="B13"/>
<contactref element="3.3V" pad="B18"/>
<contactref element="3.3V" pad="B16"/>
<contactref element="U$2" pad="7"/>
<contactref element="3.3V1" pad="A18"/>
<contactref element="3.3V1" pad="A15"/>
<contactref element="3.3V1" pad="A12"/>
<contactref element="3.3V1" pad="A4"/>
<contactref element="3.3V1" pad="B4"/>
<contactref element="3.3V1" pad="B7"/>
<contactref element="3.3V1" pad="B13"/>
<contactref element="3.3V1" pad="B18"/>
<contactref element="3.3V1" pad="B16"/>
<contactref element="X1" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="X2" pad="3"/>
<contactref element="X2" pad="2"/>
</signal>
<signal name="RX1_P">
<contactref element="U$1" pad="9"/>
<contactref element="3.3V" pad="A17"/>
</signal>
<signal name="RX1_N">
<contactref element="U$1" pad="8"/>
<contactref element="3.3V" pad="A16"/>
</signal>
<signal name="TX1_P">
<contactref element="U$1" pad="6"/>
<contactref element="3.3V" pad="B15"/>
</signal>
<signal name="TX1_N">
<contactref element="U$1" pad="5"/>
<contactref element="3.3V" pad="B14"/>
</signal>
<signal name="CLK_P">
<contactref element="U$1" pad="2"/>
<contactref element="3.3V" pad="A14"/>
</signal>
<signal name="CLK_N">
<contactref element="U$1" pad="3"/>
<contactref element="3.3V" pad="A13"/>
</signal>
<signal name="N$15">
<contactref element="U$1" pad="4"/>
<contactref element="3.3V" pad="A11"/>
</signal>
<signal name="12V">
<contactref element="3.3V" pad="A3"/>
<contactref element="3.3V" pad="A2"/>
<contactref element="3.3V" pad="B1"/>
<contactref element="3.3V" pad="B2"/>
<contactref element="3.3V" pad="B3"/>
</signal>
<signal name="N$3">
<contactref element="3.3V" pad="B11"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="3.3V" pad="A1"/>
<contactref element="3.3V" pad="B17"/>
</signal>
<signal name="N$1">
</signal>
<signal name="N$2">
</signal>
<signal name="N$4">
</signal>
<signal name="N$5">
</signal>
<signal name="3.3V">
<contactref element="3.3V" pad="A10"/>
<contactref element="3.3V" pad="A9"/>
<contactref element="3.3V" pad="B8"/>
</signal>
<signal name="RX2_P">
<contactref element="U$2" pad="6"/>
<contactref element="3.3V1" pad="A17"/>
</signal>
<signal name="RX2_N">
<contactref element="U$2" pad="5"/>
<contactref element="3.3V1" pad="A16"/>
</signal>
<signal name="TX2_P">
<contactref element="U$2" pad="9"/>
<contactref element="3.3V1" pad="B14"/>
</signal>
<signal name="TX2_N">
<contactref element="U$2" pad="8"/>
<contactref element="3.3V1" pad="B15"/>
</signal>
<signal name="CLK2_P">
<contactref element="U$2" pad="3"/>
<contactref element="3.3V1" pad="A13"/>
</signal>
<signal name="CLK2_N">
<contactref element="U$2" pad="2"/>
<contactref element="3.3V1" pad="A14"/>
</signal>
<signal name="N$7">
<contactref element="3.3V1" pad="A11"/>
<contactref element="U$2" pad="4"/>
</signal>
<signal name="3.3V1">
<contactref element="3.3V1" pad="A10"/>
<contactref element="3.3V1" pad="A9"/>
<contactref element="3.3V1" pad="B8"/>
<contactref element="X1" pad="2"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="12V1">
<contactref element="3.3V1" pad="A3"/>
<contactref element="3.3V1" pad="A2"/>
<contactref element="3.3V1" pad="B1"/>
<contactref element="3.3V1" pad="B2"/>
<contactref element="3.3V1" pad="B3"/>
<contactref element="C3" pad="1"/>
<contactref element="X2" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="3.3V1" pad="B11"/>
<contactref element="U$2" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="X1" pad="3"/>
<contactref element="C2" pad="1"/>
<contactref element="X2" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
