<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="30" y2="0" width="0" layer="20"/>
<wire x1="30" y1="0" x2="30" y2="50" width="0" layer="20"/>
<wire x1="30" y1="50" x2="0" y2="50" width="0" layer="20"/>
<wire x1="0" y1="50" x2="0" y2="0" width="0" layer="20"/>
<text>PEXternalizer Mini 0.9</text>
<text>PEXternalizer Mini 0.9
Mini PciE eXternalizer
https://github.com/
securelyfitz/PEXternalizer</text>
<text>Joe FitzPatrick
joefitz@securinghardware.com
@securelyfitz
213.373.4892</text>
</plain>
<libraries>
<library name="con-heo.mini_pci_express">
<description>&lt;b&gt;Mini PCI-Express Card&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by chris@hobbyelektronik.org&lt;/author&gt;

&lt;br&gt;&lt;br&gt;
Used PCI-SIG Specs 1.0 with addiotional information from http://www.allpinouts.org/index.php/PCI_Express_Card_and_PCI_Express_Mini_Card

&lt;br&gt;&lt;br&gt;
Made with best knowledge and conscience but errors not excluded. Please report all flaws to me - I don't want to grill any notebook.

&lt;br&gt;&lt;br&gt;

&lt;b&gt;Additional information&lt;/b&gt;
&lt;br&gt;The PCB must be 1.0mm thick. Components on top mustn't excess a height of 2.4mm and 1.35mm on bottom!</description>
<packages>
<package name="MINI_PCIE_HALF">
</package>
</packages>
</library>
<library name="con-pci_express%28pci-e%29">
<description>PCI-Express 16x  connectors, 164 contacts  (2*82)
Included: Trough-hole connector and edge-card pattern

Manufacturer: FCI  Reference: 10018783-10113TLF

Reference Radiospares: 615-9530 
Reference Digikey: 609-1975-ND</description>
<packages>
<package name="USB3_FLAT">
</package>
</packages>
</library>
<library name="securinghardware">
<packages>
<package name="SH-HALFINCH">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="con-heo.mini_pci_express" package="MINI_PCIE_HALF" value="MINI_PCIEHALF"/>
<element name="U$2" library="con-pci_express%28pci-e%29" package="USB3_FLAT" value="USB3FLAT"/>
<element name="U$3" library="securinghardware" package="SH-HALFINCH" value=""/>
<element name="U$4" library="securinghardware" package="SH-HALFINCH" value=""/>
</elements>
<signals>
<signal name="+1V5">
<contactref element="U$1" pad="28"/>
<contactref element="U$1" pad="6"/>
</signal>
<signal name="+3V3">
<contactref element="U$1" pad="52"/>
<contactref element="U$1" pad="2"/>
</signal>
<signal name="SMB_DATA">
<contactref element="U$1" pad="32"/>
</signal>
<signal name="+3V3AUX">
<contactref element="U$1" pad="24"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="HOLE1T"/>
<contactref element="U$1" pad="HOLE1B"/>
<contactref element="U$1" pad="HOLE2T"/>
<contactref element="U$1" pad="HOLE2B"/>
<contactref element="U$1" pad="43"/>
<contactref element="U$1" pad="37"/>
<contactref element="U$1" pad="35"/>
<contactref element="U$1" pad="29"/>
<contactref element="U$1" pad="27"/>
<contactref element="U$1" pad="21"/>
<contactref element="U$1" pad="15"/>
<contactref element="U$1" pad="9"/>
<contactref element="U$1" pad="4"/>
<contactref element="U$1" pad="18"/>
<contactref element="U$1" pad="26"/>
<contactref element="U$1" pad="34"/>
<contactref element="U$1" pad="40"/>
<contactref element="U$1" pad="50"/>
<contactref element="U$1" pad="7"/>
<contactref element="U$2" pad="7"/>
</signal>
<signal name="TX_P">
<contactref element="U$1" pad="33"/>
<contactref element="U$2" pad="6"/>
</signal>
<signal name="CK_P">
<contactref element="U$1" pad="13"/>
<contactref element="U$2" pad="2"/>
</signal>
<signal name="CK_N">
<contactref element="U$2" pad="3"/>
<contactref element="U$1" pad="11"/>
</signal>
<signal name="N$9">
<contactref element="U$2" pad="1"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="U$2" pad="4"/>
<contactref element="U$1" pad="22"/>
</signal>
<signal name="USB_D+">
<contactref element="U$1" pad="38"/>
</signal>
<signal name="RX_P">
<contactref element="U$2" pad="8"/>
<contactref element="U$1" pad="23"/>
</signal>
<signal name="RX_N">
<contactref element="U$1" pad="25"/>
<contactref element="U$2" pad="9"/>
</signal>
<signal name="TX_N">
<contactref element="U$1" pad="31"/>
<contactref element="U$2" pad="5"/>
</signal>
<signal name="N$1">
</signal>
</signals>
</board>
</drawing>
</eagle>
