Agilent E1733A Dimensional Metrology Software Release Notes

[Agilent E1733A 1.09]:
Bugs fixed:
1. Fixed a bug that environmental data is not saved in some cases.
2. Fixed a bug that former data is not cleared when a new setup, which is the same as before, is loaded.
3. (#95,96,97,98,106) Encoder Trigger (AqB) modified to correct trigger errors.

Upgraded:
1. Dual axes measurement is newly defined, two windows popup for each axis.
2. For dual axes, [Reset], [Start], [Record] and [Stop] buttons are sychronized for both windows.
3. Above function can be enabled/disabled by checking/unchecking "Synchronized Operation" option in system setup.
4. (#74,91,93) Merge function is added to the popup menu of open button. User can load another data file to compare with.
5. (#33) User can select numeric graph for flatness, by clicking [3D]/[2D] button on the tool bar above graph panel.
6. AqB samples are trigged in real time with no averaging to bring results closer to 5529 system.

Further modified:
1. (#123) Fixed a bug that top setup doesn't work for the first axis in linear dual axes measurement.
2. (#100,124) Preset value can be set to 0.1nm, which is the same as the highest resolution of laser position.
3. (#125) Fixed a bug that tranditional Chinese are not properly displayed in some case.
4. (#126) In AQB mode, the first data is automatically recorded when [Start] buttom is clicked, if laser position is within the target window.  First position will wait for the Auto trigger dwell time.

---------------------------------------------------------------------
[Agilent E1733A 1.08]:
Bugs fixed:
1. (#101) Fixed a bug that the end temperature is not properly printed in ISO230-2(2006) report. 

Modified:
1. Dual-Axes measurement is temporarily removed.
2. (#110) Setup forms will now pop-up at the center of the screen.
3. (#102) Added print options in Data Analysis dialog for environmental data.  Can choose Max/Min/Avg or Start/End.
   These are the same as 10747F software.
4. (#103) NDE information is not printed in ISO report if NDE correction is not used.
5. (#111) Added an extra option which allows user to modify humidity value even when air sensor is connected.

---------------------------------------------------------------------
[Agilent E1733A 1.07(Beta)]:
Bugs fixed:
1. (#31) Beam strength displays properly on 10888A remote control.

---------------------------------------------------------------------
[Agilent E1733A 1.06]:
Upgraded:
1. Added ISO 2030-2 2006 standard.

Bugs fixed:
1. Fixed a bug on displaying figure of way straightness.
2. Fixed a bug that the title of the figure of time-base measurement is not properly displayed.

Modified:
1. The driver files are updated for Agilent devices only.

---------------------------------------------------------------------
[Agilent E1733A 1.05]:
Bugs fixed:
1: Restored "The slope of both axes are remove by the value of the first axis in squareness
and parallelism(coplane)." of version 1.02

---------------------------------------------------------------------
[Agilent E1733A 1.04]:
Bugs fixed:
1. Fixed some compatibility problem of reading environmental data from legacy files.
2. Fixed a bug in squareness and parallelism when setup of second axis is changed.
3. Fixed a bug in squareness and parallelism when data is deleted.
4. Fixed display problem of squareness and parallelism.
5. Fixed some problems of printing report in Japanese.
6. Fixed a bug that data is taken after beam blocked.

Modified:
1. Values in diagnose section of setup are recalculated when measurement system is changed.
2. User standard is modified.
3. Error message will no longer popup when user records data out of target window.
4. Error value is can be displayed in upper panel for diagnose measurement.

Upgraded:
1. Units of um/m and uin/in are added to machine unit of angular measurement.
2. End point time out now works for all positional measurement: linear, diagnose, rotary and dual axes.

---------------------------------------------------------------------
[Agilent E1733A 1.03 Beta]:
Bugs fixed:
1. Fixed some item titles in ISO report.
2. Fixed a bug that status of E1736A is not properly displayed.
3. Fixed report print problems for Japanese.
4. Fixed a bug the program halts when it is started by a setup file of bad format.

Modified:
1. Axis name can be modified after measurement has started.
2. No more warning when [Stop] button is clicked.
3. Data can be erased without stopping measurement when the trigger type is manual.

Upgraded:
1. Print ISO 230-2 1988 report.

---------------------------------------------------------------------
[Agilent E1733A 1.02]:
Bugs fixed:
1. Error data of straightness measurment is recalculated immediately when slope method is changed.
2. Solved text printing problem for Japanese reports.
3. Fixed a bug in time base, which result is wrongly calculated when sigma is changed.
4. Fixed a bug that digits of target positions of second axis are not fully displayed.
5. Fixed a bug that time base measurement stops unexpected.
6. Fixed a bug that E1735A and E1736A can be select when measurement is running.
7. Fixed a bug that focus rectangle is not properly display when the measurement is running.
8. Fixed a bug that titles of numeral results are not printed in report.

Modified:
1. Grid button is still enabled when user scale is checked.
2. Slope method is always visible for squareness and parallelism
3. If use change name of axis, the title of figure is also changed correspondingly.
4. When option "Information" is checked, machine info. and ISO info. are kept when measurement is changed.
5. Strings in legacy file are translated.
6. Expan. Coef. is shown in report only for linear and related measurement types.
7. The slope of both axes are remove by the value of the first axis in squareness and parallelism(coplane).
8. Target positions of second axis can be modified when first axis is measured.
9. In way straightness, processed data are displayed instead of raw data.

Upgraded:
1. Timer trigger is added to angular/straightness measurement.
2. Saved/printed raw data can now be sorted by position or run number.
3. User can change sign of error data and targer positions.
4. Format of printed raw data is improved.

---------------------------------------------------------------------
[Agilent E1733A 1.01 Beta]:
Bugs fixed:
1. A bug of calculating compensation values.
2. A bug of displaying axis name.

Modified:
1. Maximum number of cycles is increased to 5000.
2. Raw data now can be printed directly.
3. The format of saved legacy raw data is the same as what is displayed in data grid.

---------------------------------------------------------------------
[Agilent E1733A 1.0]:
Bugs fixed:
1. Fixed a bug that target position of digonal measurement is wrongly set.

Modified:
1. Default setup is changed from "Default" to "Saved".
2. Italian is not support
3. Help function is removed.

---------------------------------------------------------------------






