Agilent N1231A Board Driver/API/Software Installation CD

This CD (or compressed file) contains the low-level hardware Driver, user Application Programming Interface DLL (API), and Demo and Development software for the Agilent N1231A PCI Laser Axis Board. This software is compatible with both 32-bit and 64-bit versions of Windows XP, Windows Vista, and Windows 7.

The New Hardware Found wizard installs the low-level Drivers and APIs using the .INF file in the Drivers\ subdirectory. See the ReadMe file for addtional information. OEMs can use the .INF and driver files contained in the zip file found in the OEM\ subdirectory.

To install the Demo and / or Development software for the Agilent N1231A Board, press the corresponding link below. Note that one should be logged in with Administrator rights and must agree to the license terms to properly install and legally use the software.

> Agilent N1231A PCI Three-Axis Board with External Sampling . . . . . . . . . . . . . . Detailed Installation Information

Note that this CD also conatains the legacy drivers and software for the above board for operation under older versions of the Microsoft Windows operating system. Click here for more information on installing this software.

Link to the Laser Interferometer section of the
Agilent Technologies web site for information on related products.

Link to the Agilent Technoligies web site .

Copyright © 2013, Agilent Technologies, Inc. All Rights Reserved.