[:SENSe]:TDSCdma:ADVanced:CHANnel:THReshold | command/query

Gets or sets the threshold above which a code channel is considered active and included in the Composite Reference waveform.

Command Syntax: | [:SENSe]:TDSCdma:ADVanced:CHANnel:THReshold <value>
<value> | ::= | Real number
Query Syntax: | [:SENSe]:TDSCdma:ADVanced:CHANnel:THReshold?
Returns | ::= | Real number
Remarks: | <none>
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Tdscdma.Interfaces.MeasurementExtension.ActiveChannelThreshold

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |