[:SENSe]:LTE:PROFile:ULINk:USER:PUSCh:ALLocation:MODulation:CW1 | command/query

Gets or sets the modulation type for Code word 1 of the allocation/channel.

Command Syntax: | [:SENSe]:LTE:PROFile:ULINk:USER[1:N]:PUSCh:ALLocation[1:N]:MODulation:CW1 <value>
<value> | ::= | "Qpsk" | "Qam16" | "Qam64"
Query Syntax: | [:SENSe]:LTE:PROFile:ULINk:USER[1:N]:PUSCh:ALLocation[1:N]:MODulation:CW1?
Returns | ::= | "Qpsk" | "Qam16" | "Qam64"
Remarks: | <none>
Example: |
    :LTE:PROF:ULIN:USER:PUSC:ALL:MOD:CW1 "Qpsk"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.AllocationBase.CW1ModType Agilent.SA.Vsa.Lte.ModulationFormatType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |