[:SENSe]:W11A:ADVanced:SUBCarrier:SPACing | command/query

Gets or sets the subcarrier spacing of the input signal.

Command Syntax: | [:SENSe]:W11A:ADVanced:SUBCarrier:SPACing <value>
<value> | ::= | Real number
Query Syntax: | [:SENSe]:W11A:ADVanced:SUBCarrier:SPACing?
Returns | ::= | Real number
Remarks: | <none>
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Wlan80211Agjp.Interfaces.MeasurementExtension.SubcarrierSpacing

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |