[:SENSe]:W16E:ADVanced:TRCK:AMPLitude | command/query

Gets or sets a value indicating whether pilot amplitude tracking is enabled.

Command Syntax: | [:SENSe]:W16E:ADVanced:TRCK:AMPLitude <value>
<value> | ::= | 0 | 1
Query Syntax: | [:SENSe]:W16E:ADVanced:TRCK:AMPLitude?
Returns | ::= | 0 | 1
Remarks: | <none>
Example: |
    :W16E:ADV:TRCK:AMPL 0
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Ieee80216Ofdma.Interfaces.MeasurementExtension.IsTrackAmplitude

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |