[:SENSe]:WCDMa[:FORMat]:PRESet | command

Preset the Wcdma measurement.

Command Syntax: | [:SENSe]:WCDMa[:FORMat]:PRESet <direction>
<direction> | ::= | "Downlink" | "Uplink"
Remarks: | <none>
Example: |
    :WCDM:PRES "Downlink"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Wcdma.Interfaces.MeasurementExtension.Preset Agilent.SA.Vsa.Wcdma.Direction

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |