[:SENSe]:LTE:ADVanced:EQUalizer:TRAining:MODE | command/query

Gets or sets the equalizer training mode (Uplink only)

Command Syntax: | [:SENSe]:LTE:ADVanced:EQUalizer:TRAining:MODE <value>
<value> | ::= | "ZF" | "LS"
Query Syntax: | [:SENSe]:LTE:ADVanced:EQUalizer:TRAining:MODE?
Returns | ::= | "ZF" | "LS"
Remarks: | <none>
Example: |
    :LTE:ADV:EQU:TRA:MODE "ZF"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.MeasurementExtension.EqualizerTrainingMode Agilent.SA.Vsa.Lte.EqualizerTrainingModeType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |