[:SENSe]:W11B[:FORMat]:MODulation:SELection | command/query

Gets or sets how the modulation format of the data part of the burst is determined.

Command Syntax: | [:SENSe]:W11B[:FORMat]:MODulation:SELection <value>
<value> | ::= | "Automatic" | "Manual"
Query Syntax: | [:SENSe]:W11B[:FORMat]:MODulation:SELection?
Returns | ::= | "Automatic" | "Manual"
Remarks: | <none>
Example: |
    :W11B:MOD:SEL "Automatic"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Wlan80211BG.Interfaces.MeasurementExtension.DataModulationSelection Agilent.SA.Vsa.Wlan80211BG.DataModulationSelection

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |