[:SENSe]:LTE:PROFile:PRS:BANDwidth | command/query

Gets or sets Positioning RS Bandwidth, N_RB^PRS.

Command Syntax: | [:SENSe]:LTE:PROFile:PRS:BANDwidth <value>
<value> | ::= | "BW1P4Mhz6RB" | "BW3Mhz15RB" | "BW5Mhz25RB" | "BW10Mhz50RB" | "BW15Mhz75RB" | "BW20Mhz100RB"
Query Syntax: | [:SENSe]:LTE:PROFile:PRS:BANDwidth?
Returns | ::= | "BW1P4Mhz6RB" | "BW3Mhz15RB" | "BW5Mhz25RB" | "BW10Mhz50RB" | "BW15Mhz75RB" | "BW20Mhz100RB"
Remarks: | <none>
Example: |
    :LTE:PROF:PRS:BAND "BW1P4Mhz6RB"
Version: | 16.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.MeasurementExtension.PositioningRsBandwidth Agilent.SA.Vsa.Lte.AnalysisBandwidthType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |