:INPut:CHANnel:CONFigure | command/query

Changes the input channel configuration for the current measurement by specifying logical channel types for the input channels.

Command Syntax: | :INPut:CHANnel:CONFigure <logicalChanArgs>
<logicalChanArgs> | ::= | Comma separated values of RF | BB | IQ | DIG | USER | EMIX
Query Syntax: | :INPut:CHANnel:CONFigure?
Returns | ::= | Comma separated values of RF | BB | IQ | DIG | USER | EMIX
Remarks: | Possible values are RF, BB, IQ, DIG, USER, EMIX (added in version 15.0). Note that if a custom configuration was specified from the GUI or the INP:CHAN:CONF:CUSTom command, the return value of this command may not provide complete details of physical to logical channel mappings. The query form of this command will return a list of channel types (comma separated) if it is a multi-channel configuration. The effect on traces is undefined for this command. The DISP:LAY, TRAC:COUN, TRAC:ADD, TRAC:REM, and TRAC:DATA:NAME commands may be useful in presetting traces to a default layout, number, and result assignment after changing the channel configuration.
Example: |
    //Setup 4 baseband channels
    INP:CHAN:CONF BB,BB,BB,BB

    //Setup Dual I+jQ
    INP:CHAN:CONF IQ,IQ

    //Setup single RF
    INP:CHAN:CONF RF
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.Input.ChangeLogicalChannels

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |