[:SENSe]:W11N:ADVanced:TRCK:MODE | command/query

Gets or sets how pilot tracking is done for MIMO signals.

Command Syntax: | [:SENSe]:W11N:ADVanced:TRCK:MODE <value>
<value> | ::= | "PostEqualizer" | "PreEqualizer"
Query Syntax: | [:SENSe]:W11N:ADVanced:TRCK:MODE?
Returns | ::= | "PostEqualizer" | "PreEqualizer"
Remarks: | <none>
Example: |
    :W11N:ADV:TRCK:MODE "PostEqualizer"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Wlan80211N.Interfaces.MeasurementExtension.TrackMode Agilent.SA.Vsa.Wlan80211N.TrackMode

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |