[:SENSe]:LTE[:FORMat]:DLINk:PATH:INACtive | command/query

Gets or sets a value indicating whether antenna paths below the antenna detection threshold (-36 dB default) in power from the reference antenna path are shown or blanked on the MIMO traces.

Command Syntax: | [:SENSe]:LTE[:FORMat]:DLINk:PATH:INACtive <value>
<value> | ::= | 0 | 1
Query Syntax: | [:SENSe]:LTE[:FORMat]:DLINk:PATH:INACtive?
Returns | ::= | 0 | 1
Remarks: | <none>
Example: |
    :LTE:DLIN:PATH:INAC 0
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.MeasurementExtension.IsIncludeInactivePathsEnabled

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |