[:SENSe]:FREQuency:SPAN:DEFault | command

Sets the Span to its default value, which is the largest span supported by the current hardware.

Command Syntax: | [:SENSe]:FREQuency:SPAN:DEFault
Remarks: | <none>
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.Frequency.DefaultSpan

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |