[:SENSe]:CUSTomofdm[:FORMat]:PRESet | command

Preset the CustomOfdm measurement.

Command Syntax: | [:SENSe]:CUSTomofdm[:FORMat]:PRESet <standard>
<standard> | ::= | "Ieee80211A" | "DabModeI" | "DabModeII" | "DabModeIII" | "DabModeIV" | "DvbTH2K" | "DvbTH4K" | "DvbTH8K" | "DvbSH1K" | "IsdbTMode3A1B12"
Remarks: | <none>
Example: |
    :CUST:PRES "Ieee80211A"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.CustomOfdm.Interfaces.MeasurementExtension.Preset Agilent.SA.Vsa.CustomOfdm.Standard

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |