[:SENSe]:W16E:MIMO:CHANnel | command/query

Gets or sets the STC/MIMO input measurement channel.

Command Syntax: | [:SENSe]:W16E:MIMO:CHANnel <value>
<value> | ::= | "Chan1" | "Chan2"
Query Syntax: | [:SENSe]:W16E:MIMO:CHANnel?
Returns | ::= | "Chan1" | "Chan2"
Remarks: | <none>
Example: |
    :W16E:MIMO:CHAN "Chan1"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Ieee80216Ofdma.Interfaces.MeasurementExtension.InputChannel Agilent.SA.Vsa.Ieee80216Ofdma.InputChannelType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |