[:SENSe]:W11B:ADVanced:EQUalize:FILTer[:LENGth] | command/query

Gets or sets the filter length of the equalizer. This is the length of the equalizer impulse response.

Command Syntax: | [:SENSe]:W11B:ADVanced:EQUalize:FILTer[:LENGth] <value>
<value> | ::= | Integer number
Query Syntax: | [:SENSe]:W11B:ADVanced:EQUalize:FILTer[:LENGth]?
Returns | ::= | Integer number
Remarks: | <none>
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Wlan80211BG.Interfaces.MeasurementExtension.EqualizerFilterLength

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |