[:SENSe]:RBW:POINts:AUTO | command/query

Gets or sets a value indicating whether the number of frequency points is automatically adjusted to accommodate a larger range of ResBW values (and correspondingly, time record lengths).

Command Syntax: | [:SENSe]:RBW:POINts:AUTO <value>
<value> | ::= | 0 | 1
Query Syntax: | [:SENSe]:RBW:POINts:AUTO?
Returns | ::= | 0 | 1
Remarks: | <none>
Example: |
    :RBW:POIN:AUTO 0
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.Frequency.IsPointsAuto

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |