[:SENSe]:W11N:STANdard | command/query

Gets or sets the signal standard used by the transmitter.

Command Syntax: | [:SENSe]:W11N:STANdard <value>
<value> | ::= | "Ieee80211Nac20" | "Ieee80211N20" | "Ieee80211Nac40" | "Ieee80211N40" | "Ieee80211AC80" | "Ieee80211AC80Plus80" | "Ieee80211AC160"
Query Syntax: | [:SENSe]:W11N:STANdard?
Returns | ::= | "Ieee80211Nac20" | "Ieee80211N20" | "Ieee80211Nac40" | "Ieee80211N40" | "Ieee80211AC80" | "Ieee80211AC80Plus80" | "Ieee80211AC160"
Remarks: | <none>
Example: |
    :W11N:STAN "Ieee80211Nac20"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Wlan80211N.Interfaces.MeasurementExtension.Standard Agilent.SA.Vsa.Wlan80211N.Standard

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |