[:SENSe]:W16E:TIME:SYNC:OFFSet | command/query

Gets or sets the start of the window for uplink synchronization (in symbols) relative to the pulse search if enabled, or trigger otherwise.

Command Syntax: | [:SENSe]:W16E:TIME:SYNC:OFFSet <value>
<value> | ::= | Real number
Query Syntax: | [:SENSe]:W16E:TIME:SYNC:OFFSet?
Returns | ::= | Real number
Remarks: | <none>
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Ieee80216Ofdma.Interfaces.MeasurementExtension.SynchronizationSearchOffset

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |