[:SENSe]:LTE:PROFile:MBSFn:PMCH:MODulation | command/query

Gets or sets the mod type of the PMCH contained in each of 10 subframe

Command Syntax: | [:SENSe]:LTE:PROFile:MBSFn:PMCH:MODulation <modFormats>
<modFormats> | ::= | Comma separated values of "Qpsk" | "Qam16" | "Qam64"
Query Syntax: | [:SENSe]:LTE:PROFile:MBSFn:PMCH:MODulation?
Returns | ::= | Comma separated values of "Qpsk" | "Qam16" | "Qam64"
Remarks: | <none>
Example: |
    :LTE:PROF:MBSF:PMCH:MOD “Qpsk”,“Qpsk”,“Qpsk”,“Qpsk","Qam16","Qam16","Qam16","Qam64","Qam64","Qam64"
Version: | 16.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.MeasurementExtension.SetPmchModType Agilent.SA.Vsa.Lte.ModulationFormatType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |