[:SENSe]:W11N:ADVanced:FFTLength | command/query

Gets or sets the FFT length for the measurement.

Command Syntax: | [:SENSe]:W11N:ADVanced:FFTLength <value>
<value> | ::= | "Points64" | "Points128" | "Points256" | "Points512"
Query Syntax: | [:SENSe]:W11N:ADVanced:FFTLength?
Returns | ::= | "Points64" | "Points128" | "Points256" | "Points512"
Remarks: | <none>
Example: |
    :W11N:ADV:FFTL "Points64"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Wlan80211N.Interfaces.MeasurementExtension.FftLength Agilent.SA.Vsa.Wlan80211N.FftLength

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |