[:SENSe]:RFID:ADVanced:THReshold:ASK:UPPer | command/query

Gets or sets the ASK upper pulse threshold.

Command Syntax: | [:SENSe]:RFID:ADVanced:THReshold:ASK:UPPer <value>
<value> | ::= | Real number
Query Syntax: | [:SENSe]:RFID:ADVanced:THReshold:ASK:UPPer?
Returns | ::= | Real number
Remarks: | <none>
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Rfid.Interfaces.MeasurementExtension.AskPulseUpperThreshold

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |