[:SENSe]:LTE:PROFile:PHICh:DURation | command/query

Gets or sets the PHICH Duration mode as being auto-detected, normal or extended.

Command Syntax: | [:SENSe]:LTE:PROFile:PHICh:DURation <value>
<value> | ::= | "Auto" | "Normal" | "Extended"
Query Syntax: | [:SENSe]:LTE:PROFile:PHICh:DURation?
Returns | ::= | "Auto" | "Normal" | "Extended"
Remarks: | <none>
Example: |
    :LTE:PROF:PHIC:DUR "Auto"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.MeasurementExtension.PhichDurationMode Agilent.SA.Vsa.Lte.PhichDurationType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |