[:SENSe]:LTE:ADVanced:ULINk:CCONdition | command/query

Gets or sets the channel condition to be used for spectral flatness test as normal or extreme.

Command Syntax: | [:SENSe]:LTE:ADVanced:ULINk:CCONdition <value>
<value> | ::= | "Normal" | "Extreme"
Query Syntax: | [:SENSe]:LTE:ADVanced:ULINk:CCONdition?
Returns | ::= | "Normal" | "Extreme"
Remarks: | <none>
Example: |
    :LTE:ADV:ULIN:CCON "Normal"
Version: | 16.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.MeasurementExtension.ChannelCondition Agilent.SA.Vsa.Lte.ChannelConditionType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |