:TRACe:MARKer:BANDwidth:TYPE | command/query

Gets or sets the Band Power base calculation (either power or density values).

Command Syntax: | :TRACe[1:N]:MARKer[1:N]:BANDwidth:TYPE <bandType>
<bandType> | ::= | "Power" | "Density"
Query Syntax: | :TRACe[1:N]:MARKer[1:N]:BANDwidth:TYPE?
Returns | ::= | "Power" | "Density"
Remarks: | <none>
Example: |
    :TRAC:MARK:BAND:TYPE "Power"
Version: | 13.01 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.Marker.BandType Agilent.SA.Vsa.MarkerBandType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |