[:SENSe]:WCDMa:ADVanced:MIMO:FREQuency:OFFSet | command/query

Gets or sets where frequency offset is assumed to originate in the analyzed MIMO signal.

Command Syntax: | [:SENSe]:WCDMa:ADVanced:MIMO:FREQuency:OFFSet <value>
<value> | ::= | "Transmitter" | "Receiver"
Query Syntax: | [:SENSe]:WCDMa:ADVanced:MIMO:FREQuency:OFFSet?
Returns | ::= | "Transmitter" | "Receiver"
Remarks: | <none>
Example: |
    :WCDM:ADV:MIMO:FREQ:OFFS "Transmitter"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Wcdma.Interfaces.MeasurementExtension.MimoFrequencyOffsetModel Agilent.SA.Vsa.Wcdma.MimoImpairmentModel

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |