[:SENSe]:DDEMod:ADVanced:CPMindex:AUTO | command/query

Gets or sets a value indicating whether CPM (Continuous Phase Modulation) values for {h1, h2} (modulation index values) are auto-detected.

Command Syntax: | [:SENSe]:DDEMod:ADVanced:CPMindex:AUTO <value>
<value> | ::= | 0 | 1
Query Syntax: | [:SENSe]:DDEMod:ADVanced:CPMindex:AUTO?
Returns | ::= | 0 | 1
Remarks: | <none>
Example: |
    :DDEM:ADV:CPM:AUTO 0
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.DigitalDemod.Interfaces.MeasurementExtension.IsCpmIndexAuto

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |