[:SENSe]:LTE[:FORMat]:DLINk:TXANtenna:REFerence:PORT | command/query

Gets or sets the TX antenna port to be used as the reference antenna port

Command Syntax: | [:SENSe]:LTE[:FORMat]:DLINk:TXANtenna:REFerence:PORT <value>
<value> | ::= | "Port0" | "Port1" | "Port2" | "Port3" | "Port4" | "Port5" | "Port6" | "Port7" | "Port8"
Query Syntax: | [:SENSe]:LTE[:FORMat]:DLINk:TXANtenna:REFerence:PORT?
Returns | ::= | "Port0" | "Port1" | "Port2" | "Port3" | "Port4" | "Port5" | "Port6" | "Port7" | "Port8"
Remarks: | <none>
Example: |
    :LTE:DLIN:TXAN:REF:PORT "Port0"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.MeasurementExtension.TXAntenna Agilent.SA.Vsa.Lte.AntennaPortType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |