[:SENSe]:WCDMa[:FORMat]:SYNC:SLOT:STARt | command/query

Gets or sets which slot within a frame should be the first analysis slot.

Command Syntax: | [:SENSe]:WCDMa[:FORMat]:SYNC:SLOT:STARt <value>
<value> | ::= | Integer number
Query Syntax: | [:SENSe]:WCDMa[:FORMat]:SYNC:SLOT:STARt?
Returns | ::= | Integer number
Remarks: | <none>
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Wcdma.Interfaces.MeasurementExtension.SynchronizationStartSlot

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |