[:SENSe]:TDSCdma:ADVanced:CHANnel:THReshold:AUTO | command/query

Gets or sets a value indicating whether active channel threshold is automatically detected.

Command Syntax: | [:SENSe]:TDSCdma:ADVanced:CHANnel:THReshold:AUTO <value>
<value> | ::= | 0 | 1
Query Syntax: | [:SENSe]:TDSCdma:ADVanced:CHANnel:THReshold:AUTO?
Returns | ::= | 0 | 1
Remarks: | <none>
Example: |
    :TDSC:ADV:CHAN:THR:AUTO 0
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Tdscdma.Interfaces.MeasurementExtension.IsActiveChannelThresholdAutomatic

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |