[:SENSe]:C2K[:FORMat]:PRESet | command

Preset the cdma2000 measurement.

Command Syntax: | [:SENSe]:C2K[:FORMat]:PRESet <direction>
<direction> | ::= | "Forward" | "Reverse"
Remarks: | <none>
Example: |
    :C2K:PRES "Forward"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Cdma2000.Interfaces.MeasurementExtension.Preset Agilent.SA.Vsa.Cdma2000.Direction

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |