[:SENSe]:LTE:PROFile:PRS:PRECoding | command/query

Gets or sets whether the signal has precoding applied to the Positioning RS resource elements.

Command Syntax: | [:SENSe]:LTE:PROFile:PRS:PRECoding <value>
<value> | ::= | "Off" | "On"
Query Syntax: | [:SENSe]:LTE:PROFile:PRS:PRECoding?
Returns | ::= | "Off" | "On"
Remarks: | <none>
Example: |
    :LTE:PROF:PRS:PREC "Off"
Version: | 16.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.MeasurementExtension.PositioningRsPrecoding Agilent.SA.Vsa.Lte.PositioningRsPrecodingType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |