[:SENSe]:LTE:ADVanced:UERS:COMPensate:WEIGht:DISPlay | command/query

Gets or sets how the UE-specific RS weights are displayed in the UE-specific RS weights table.

Command Syntax: | [:SENSe]:LTE:ADVanced:UERS:COMPensate:WEIGht:DISPlay <value>
<value> | ::= | "PerSubcarrier" | "PerRB" | "PerUser"
Query Syntax: | [:SENSe]:LTE:ADVanced:UERS:COMPensate:WEIGht:DISPlay?
Returns | ::= | "PerSubcarrier" | "PerRB" | "PerUser"
Remarks: | <none>
Example: |
    :LTE:ADV:UERS:COMP:WEIG:DISP "PerSubcarrier"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.MeasurementExtension.UersWeightsDisplayMode Agilent.SA.Vsa.Lte.UersWeightsDisplayModeType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |