[:SENSe]:LTE:PROFile:ULINk:USER:PUSCh:COUPling:RB:END | command/query

Gets or sets a value indicating whether all the allocations share the same RB End.

Command Syntax: | [:SENSe]:LTE:PROFile:ULINk:USER[1:N]:PUSCh:COUPling:RB:END <value>
<value> | ::= | 0 | 1
Query Syntax: | [:SENSe]:LTE:PROFile:ULINk:USER[1:N]:PUSCh:COUPling:RB:END?
Returns | ::= | 0 | 1
Remarks: | <none>
Example: |
    :LTE:PROF:ULIN:USER:PUSC:COUP:RB:END 0
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.Channel.IsRBEndCoupled

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |