[:SENSe]:W16D:ADVanced:SCHannel:INDex | command/query

Gets or sets the subchannel index for uplink signals.

Command Syntax: | [:SENSe]:W16D:ADVanced:SCHannel:INDex <value>
<value> | ::= | Integer number
Query Syntax: | [:SENSe]:W16D:ADVanced:SCHannel:INDex?
Returns | ::= | Integer number
Remarks: | <none>
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Ieee80216Ofdm.Interfaces.MeasurementExtension.SubchannelIndex

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |