:INPut:ANALog:IMPedance:REFerence:CONNection:CHANnel | command/query

Gets or sets a value indicating whether the reference impedance follows the connector impedance.

Command Syntax: | :INPut:ANALog:IMPedance:REFerence:CONNection:CHANnel[1:N] <isConnection>
<isConnection> | ::= | 0 | 1
Query Syntax: | :INPut:ANALog:IMPedance:REFerence:CONNection:CHANnel[1:N]?
Returns | ::= | 0 | 1
Remarks: | <none>
Example: |
    :INP:ANAL:IMP:REF:CONN:CHAN 0
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.AnalogChannel.RefImpedanceIsConnection

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |