[:SENSe]:W11N[:FORMat]:STReams:SELection | command/query

Gets or sets how the number of spatial streams is determined.

Command Syntax: | [:SENSe]:W11N[:FORMat]:STReams:SELection <value>
<value> | ::= | "Automatic" | "Manual" | "Sig" | "HTSig"
Query Syntax: | [:SENSe]:W11N[:FORMat]:STReams:SELection?
Returns | ::= | "Automatic" | "Manual" | "Sig" | "HTSig"
Remarks: | <none>
Example: |
    :W11N:STR:SEL "Automatic"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Wlan80211N.Interfaces.MeasurementExtension.StreamsSelection Agilent.SA.Vsa.Wlan80211N.StreamsSelection

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |