[:SENSe]:LTE[:FORMat]:SYNCtype | command/query

Gets or sets the channel to synchronize to.

Command Syntax: | [:SENSe]:LTE[:FORMat]:SYNCtype <value>
<value> | ::= | "Psch" | "RS" | "PucchRS" | "Srs" | "Prach"
Query Syntax: | [:SENSe]:LTE[:FORMat]:SYNCtype?
Returns | ::= | "Psch" | "RS" | "PucchRS" | "Srs" | "Prach"
Remarks: | Valid values are different depending on whether the LTE:DIRection is uplink or downlink. See related .NET command link for details.
Example: |
    :LTE:SYNC "Psch"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.MeasurementExtension.SynchronizationType Agilent.SA.Vsa.Lte.SynchronizationTypeSelection

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |