[:SENSe]:LTE:ADVanced:UERS:COMPensate | command/query

Gets or sets a value indicating whether channel response is compensated from UE-RS weights

Command Syntax: | [:SENSe]:LTE:ADVanced:UERS:COMPensate <value>
<value> | ::= | 0 | 1
Query Syntax: | [:SENSe]:LTE:ADVanced:UERS:COMPensate?
Returns | ::= | 0 | 1
Remarks: | <none>
Example: |
    :LTE:ADV:UERS:COMP 0
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.MeasurementExtension.IsUersChannelResponseCompensationEnabled

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |