[:SENSe]:LTE:PROFile:DLINk:USER:UERS:NSCRambling:ID | command/query

Gets or sets the n_SCID for the generation of UE-specific RS for the DL user.

Command Syntax: | [:SENSe]:LTE:PROFile:DLINk:USER[1:N]:UERS:NSCRambling:ID <value>
<value> | ::= | "Id0" | "Id1"
Query Syntax: | [:SENSe]:LTE:PROFile:DLINk:USER[1:N]:UERS:NSCRambling:ID?
Returns | ::= | "Id0" | "Id1"
Remarks: | <none>
Example: |
    :LTE:PROF:DLIN:USER:UERS:NSCR:ID "Id0"
Version: | 14.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.DownlinkUser.UersNScramblingId Agilent.SA.Vsa.Lte.UersScramblingId

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |