[:SENSe]:GSM[:FORMat]:BURSttype | command/query

Gets or sets the Burst Types that the measurement will consider for demodulation.

Command Syntax: | [:SENSe]:GSM[:FORMat]:BURSttype <value>
<value> | ::= | "Normal" | "HighSymbolRate" | "Mixed" | "Access" | "Synchronization"
Query Syntax: | [:SENSe]:GSM[:FORMat]:BURSttype?
Returns | ::= | "Normal" | "HighSymbolRate" | "Mixed" | "Access" | "Synchronization"
Remarks: | <none>
Example: |
    :GSM:BURS "Normal"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.GsmEdgeEvolution.Interfaces.MeasurementExtension.BurstType Agilent.SA.Vsa.GsmEdgeEvolution.BurstType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |