[:SENSe]:LTE:PROFile:PHICh:ALLocation | command/query

Gets or sets the PHICH Allocation size to be used for PHICH resource element group mappings.

Command Syntax: | [:SENSe]:LTE:PROFile:PHICh:ALLocation <value>
<value> | ::= | "Auto" | "Value1By6" | "Value1By2" | "Value1" | "Value2"
Query Syntax: | [:SENSe]:LTE:PROFile:PHICh:ALLocation?
Returns | ::= | "Auto" | "Value1By6" | "Value1By2" | "Value1" | "Value2"
Remarks: | <none>
Example: |
    :LTE:PROF:PHIC:ALL "Auto"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.MeasurementExtension.PhichAllocation Agilent.SA.Vsa.Lte.PhichAllocationType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |