[:SENSe]:LTE:PROFile:ULINk:USER:PRACh:MODulation | command/query

Gets or sets the modulation type for the allocation/channel.

Command Syntax: | [:SENSe]:LTE:PROFile:ULINk:USER[1:N]:PRACh:MODulation <value>
<value> | ::= | "Qpsk" | "Qam16" | "Qam64"
Query Syntax: | [:SENSe]:LTE:PROFile:ULINk:USER[1:N]:PRACh:MODulation?
Returns | ::= | "Qpsk" | "Qam16" | "Qam64"
Remarks: | <none>
Example: |
    :LTE:PROF:ULIN:USER:PRAC:MOD "Qpsk"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.AllocationBase.ModType Agilent.SA.Vsa.Lte.ModulationFormatType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |