[:SENSe]:INPut:CORRection:CONStant:DCOFfset | command/query

Gets or sets the DC offset added (in Volts) to an input channel.

Command Syntax: | [:SENSe]:INPut:CORRection[1:N]:CONStant:DCOFfset <dcOffset>
<dcOffset> | ::= | Real number
Query Syntax: | [:SENSe]:INPut:CORRection[1:N]:CONStant:DCOFfset?
Returns | ::= | Real number
Remarks: | <none>
Version: | 16.20 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.InputCorrection.DCOffset

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |