[:SENSe]:W16E:ZONE:ULINk:ACTive[:ZONE] | command

Gets or sets a value indicating whether the zone is active for analysis.

Command Syntax: | [:SENSe]:W16E:ZONE:ULINk:ACTive[:ZONE] <zone>
<zone> | ::= | String
Remarks: | <none>
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Ieee80216Ofdma.Interfaces.UplinkZone.IsActive

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |