:INPut:CHANnel:CONFigure:CUSTom | command/query

Changes the input channel configuration for the current measurement by specifying logical channel types for the input channels.

Command Syntax: | :INPut:CHANnel:CONFigure:CUSTom
Query Syntax: | :INPut:CHANnel:CONFigure:CUSTom?
Returns | ::= | String
Remarks: | <none>
Example: |
    //4 channels custom logical-physical mapping
    INP:CHAN:CONF:CUST "1,3,2,4"

    //Dual I+jQ with specific channel mapping
    INP:CHAN:CONF:CUST "IQ_1_3,IQ_2_4"

    //Specify 2 RF channels on dual signal analyzers
    INP:CHAN:CONF:CUST "1.1,2.1"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.Input.ChangeLogicalChannels

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |