:INPut:TRIGger:FMASk:RBW | command/query

Gets or sets the resolution bandwidth.

Command Syntax: | :INPut:TRIGger:FMASk:RBW <value>
<value> | ::= | Real number
Query Syntax: | :INPut:TRIGger:FMASk:RBW?
Returns | ::= | Real number
Remarks: | <none>
Version: | 17.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.FrequencyMaskTrigger.ResBW

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |